# Static Call Analysis for
loadapp (MAIN_B)

Created from: LX51 LINKER/LOCATER V4.00 BETA
Creation time: 08/31/2005 15:30:50

## ?PR?MAIN?MAIN_B (8000F3H - 80011BH)

Maximum Stack: Bottom=9 Bytes (?PR?MAIN_APP?MAIN_A)

Calls to:

- ?L?COM0001
- ?PR?INT_OFF?MAIN_B
- ?PR?INT_ON?MAIN_B
- ?PR?MAIN_APP?MAIN_A
- ?PR?T2_INI_LOAD?MAIN_B

## ?PR?TIMER2?INT (800130H - 800158H)

Maximum Stack: Bottom=14 Bytes (?PR?T2_ISR_LOAD?MAIN_B)

Calls to:

- ?PR?T2_ISR_APP?MAIN_A
- ?PR?T2_ISR_LOAD?MAIN_B

Called from:

- ?INT?0002B

## ?INT?0002B (80002BH - 80002CH)

Maximum Stack: Bottom=14 Bytes (?PR?TIMER2?INT)

Calls to:

- ?PR?TIMER2?INT

## ?PR?T2_INI_LOAD?MAIN_B (80011FH - 800129H)

Maximum Stack: Bottom=3 Bytes (?L?COM0005) Top=3 Bytes (?PR?MAIN?MAIN_B)

Calls to:

- ?L?COM0004
- ?L?COM0005

Called from:

- ?PR?MAIN?MAIN_B

## ?PR?T2_ISR_LOAD?MAIN_B (80012DH - 80012FH)

Maximum Stack: Bottom=3 Bytes (?L?COM0003) Top=11 Bytes (?PR?TIMER2?INT)

Calls to:

- ?L?COM0003

Called from:

- ?PR?TIMER2?INT

## ?PR?INT_ON?MAIN_B (80011CH - 80011EH)

Maximum Stack: Top=6 Bytes (?PR?MAIN_APP?MAIN_A)

Called from:

- ?PR?MAIN?MAIN_B
- ?PR?MAIN_APP?MAIN_A

## ?PR?INT_OFF?MAIN_B (80012AH - 80012CH)

Maximum Stack: Top=6 Bytes (?PR?MAIN_APP?MAIN_A)

Called from:

- ?PR?MAIN?MAIN_B
- ?PR?MAIN_APP?MAIN_A

## ?PR?MAIN_APP?MAIN_A (870000H - 87001EH)

Maximum Stack: Bottom=6 Bytes (?PR?T2_INI_APP?MAIN_A) Top=3 Bytes (?PR?MAIN?MAIN_B)

Calls to:

- ?L?COM0001
- ?PR?INT_OFF?MAIN_B
- ?PR?INT_ON?MAIN_B
- ?PR?T2_INI_APP?MAIN_A

Called from:

- ?PR?MAIN?MAIN_B

## ?PR?T2_INI_APP?MAIN_A (87001FH - 87002FH)

Maximum Stack: Bottom=3 Bytes (?L?COM0005) Top=6 Bytes (?PR?MAIN_APP?MAIN_A)

Calls to:

- ?L?COM0004
- ?L?COM0005

Called from:

- ?PR?MAIN_APP?MAIN_A

## ?PR?T2_ISR_APP?MAIN_A (870030H - 870035H)

Maximum Stack: Bottom=3 Bytes (?L?COM0003) Top=11 Bytes (?PR?TIMER2?INT)

Calls to:

- ?L?COM0003

Called from:

- ?PR?TIMER2?INT

## ?L?COM0001 (80000CH - 80001DH)

Maximum Stack: Top=6 Bytes (?PR?MAIN_APP?MAIN_A)

Called from:

- ?PR?MAIN?MAIN_B
- ?PR?MAIN_APP?MAIN_A

## ?L?COM0003 (80001EH - 800029H)

Maximum Stack: Top=14 Bytes (?PR?T2_ISR_LOAD?MAIN_B)

Called from:

- ?PR?T2_ISR_APP?MAIN_A
- ?PR?T2_ISR_LOAD?MAIN_B

## ?L?COM0004 (8000E0H - 8000EAH)

Maximum Stack: Top=9 Bytes (?PR?T2_INI_APP?MAIN_A)

Called from:

- ?PR?T2_INI_APP?MAIN_A
- ?PR?T2_INI_LOAD?MAIN_B

## ?L?COM0005 (8000EBH - 8000F2H)

Maximum Stack: Top=9 Bytes (?PR?T2_INI_APP?MAIN_A)

Called from:

- ?PR?T2_INI_APP?MAIN_A
- ?PR?T2_INI_LOAD?MAIN_B